**PCB specifications:**

Type of material: Rogers RO3010

Thickness: 1.5 mm

Board size: 38.1 x 35.6 mm (1.5 x 1.4 inch)

Quantity: 10 pcs

Conductive Layers: 2

Min track/spacing: 6 mil

Min hole size: >0.3 mm

Solder mask: none

Silkscreen: none

Surface Finish: Immersion gold

Copper layer: 1 oz

**File list:**

|  |  |
| --- | --- |
| Filename | Description |
| UTCPW\_MountingBoard-B\_Cu.gbr |  |
| UTCPW\_MountingBoard-B\_Mask.gbr |  |
| UTCPW\_MountingBoard-B\_Paste.gbr |  |
| UTCPW\_MountingBoard-Edge\_Cuts.gbr |  |
| UTCPW\_MountingBoard-F\_Cu.gbr |  |
| UTCPW\_MountingBoard-F\_Mask.gbr |  |
| UTCPW\_MountingBoard-F\_Paste.gbr |  |
| UTCPW\_MountingBoard-NPTH.drl |  |
| UTCPW\_MountingBoard-PTH.drl |  |
| UTCPW\_MountingBoard-User\_Eco1.gbr |  |
| UTCPW\_MountingBoard-job.gbrjob |  |